A picture containing shape

Description automatically generated

**Checklist for Workplace Inspection**

Names of People Conducting the Inspection:

DATE:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | (O) Good  (X) Require Action | | Room Location | Corrective Action |  | (O) Good  (X) Requires Action | Room Location | Corrective Action |
| **Air Quality** | | | | | **Electrical** | | | |
| Carpet excessively dirty stained, water damaged |  | |  |  | Emergency lights not working. Inadequate lighting creating trip hazard |  |  |  |
| Dirty air diffusers observed at ceiling |  | |  |  | Extension cords used as permanent wiring |  |  |  |
| Evidence of water leaks |  | |  |  | Power bars daisy chained |  |  |  |
| Evidence of industrial emissions, exhaust fumes |  | |  |  | Electrical baseboard heater cover missing |  |  |  |
| Heating/ventilation/exhaust system does not seem to be working |  | |  |  | Electrical baseboard heater cover missing |  |  |  |
| Offensive odor of unknown source |  | |  |  | Electrical outlet loose in the electrical box/wall |  |  |  |
| Staff expressed concern about air quality in this area |  | |  |  | Electrocution hazard |  |  |  |
| Ventilation grills blocked by material or equipment |  | |  |  | Electrical wires are cut or frayed |  |  |  |
| **Building** | | | | | High voltage sources not labelled |  |  |  |
| Ceiling tile – broken/stained/loose/missing |  | |  |  | Recessed floor outlets in need of repair |  |  |  |
| Door – knob or latch needs repair/broken |  | |  |  | Additional space heaters/microwave/fridge/kettle |  |  |  |
| Paint flaking off ceiling or walls |  | |  |  | Items hanging from ceiling light fixtures |  |  |  |
| Sink drain leaking or plugged |  | |  |  |  |  |  |  |
| Temperature extreme –either too high or low |  | |  |  | **Storage** | | | |
| Use of portable heater indicative of heating problem |  | |  |  | Bookshelf over 5ft high not secured to wall, tip hazard |  |  |  |
| Uneven treads and risers create trip hazards |  | |  |  | Improper Storage – stacked too high – tip hazard |  |  |  |
| Water damage identified |  | |  |  | Heavy items stored on top of cupboards |  |  |  |
| Windows damaged or leaking in need of repair |  | |  |  | Sharps not disposed of in approved containers |  |  |  |
| Windows damaged or leaking in need of repair |  | |  |  | **Fire Safety** | | | |
| Washroom area is unclean and lack supplies |  | |  |  | Combustibles stored in the stairwells |  |  |  |
| Washrooms fixtures in need of repair | |  |  |  | Emergency lighting not in working condition/Fire exit sign not illuminated |  |  |  |
| Drywall - open area/broken in need of repair |  | |  |  | Materials obstructing sprinkler heads |  |  |  |
| Missing signage/name plates/replace sign |  | |  |  | Door propped open against policy |  |  |  |
|  |  | |  |  | Fire exit are blocked/doors open into a hazardous area |  |  |  |
| Fire extinguishers inspection tag missing |  |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | (O) Good  (X) Requires Action | | Room Location | | Corrective Action |  | | (O) Good  (X) Requires Action | | Room Location | Corrective Action |
| **Miscellaneous** | | | | | | | **Hazard Controls** | | | | | |
| Item blocking exits, cables on the floor | |  | |  | |  | Machines guarding not in place and is not adjusted appropriately | |  | |  |  |
| Employee concern about hazard | |  | |  | |  | Chemicals - SDS Information not available, labels are missing | |  | |  |  |
| Evidence of pest (insect, rodent, etc.) | |  | |  | |  | Eye wash station inaccessible | |  | |  |  |
| First Aid – First Aid kit monthly tag outdated | |  | |  | |  | Eyewash/shower not in good working order | |  | |  |  |
| Furniture broken or in disrepair | |  | |  | |  | Fume hood -not good working order, updated tag and used for storage | |  | |  |  |
| H&S bulletin board not up to date | |  | |  | |  | PPE Signage – Not visible and is not being respected | |  | |  |  |
| General office/classroom space unclean area | |  | |  | |  |  |  | |  | |  |
| Overflowing garbage | |  | |  | |  |  | |  | |  |  |
| Walkways are blocked by clutter | |  | |  | |  | **Slips, Trips and Falls** | | | | | |
| Safety phones operational | |  | |  | |  | Change in elevation along walkway creating a trip hazard | |  | |  |  |
|  | |  | |  | |  | Electrical cords in doorways/walkways creating a trip hazard | |  | |  |  |
| **Chemical** | | | | | | | Fixed access ladder in need of repair |  | |  | |  |
| Compressed gas cylinders not stored securely to prevent falling |  | |  | |  | | Floor tiles damaged or missing, creating a trip hazard |  | |  | |  |
| Containers of chemical not closed |  | |  | |  | | Handrails loose/not secured and grip strips worn or damaged on stairs |  | |  | |  |
| Excess storage of chemicals that have expired or are no longer required |  | |  | |  | | Inadequate lighting creating trip hazard |  | |  | |  |
| Chemicals stored inappropriately |  | |  | |  | | Poor housekeeping creating a fall hazard |  | |  | |  |
| Labels missing for consumer product |  | |  | |  | | Ripped or stretched carpeting creating a trip hazard |  | |  | |  |
| **COVID-19** | | | | | | | Slip/Trip hazard general |  | |  | |  |
| SWPs and appropriate COVID signage is posted in HHLs on Safety Information Station |  | |  | |  | | Stairs/landing damaged, creating a trip hazard |  | |  | |  |
| Furniture arranged to support Physical Distancing. |  | |  | |  | | Winter slip hazards accumulation of ice and/or snow on walkways |  | |  | |  |
| Sanitation stations available or nearby |  | |  | |  | |  |  | |  | |  |
| Appropriate signage and directional indicators |  | |  | |  | |  |  | |  | |  |
| Physical barriers are in good shape |  | |  | |  | |  |  | |  | |  |
| Vista Sign for room Occupancy Limit |  | |  | |  | |  |  | |  | |  |